**Time flow cartridge**

Mechanism for TEMPOSTOP basin

Time flow ~7 seconds

Reference: **743005**

Specification description

Time flow cartridge for TEMPOSTOP basin mixers and taps.

Old version.

With push-button.

Time flow ~7 seconds.

Adjustable flow rate from 1.4 to 6 lpm