**Time flow cartridge**

Mechanism for TEMPOSOFT 2 urinal

~3sec time flow

Reference: **743744**

Specification description

Time flow cartridge for TEMPOSOFT 2 urinal valve.

For urinal valves with soft-touch operation.

For 1/2" urinal valves.

Time flow ~3 seconds.

Flow rate can be adjusted.