**TEMPOSTOP AB**

For TEMPOSTOP AB

Time flow ~ 7 seconds

Reference: **747122L**

Specification description

Time flow anti-blocking valve for cross wall TEMPOSTOP AB.

Time flow ~ 7 seconds.