**Ø35mm ceramic sequential cartridge**

Cartridge with base and collar

Reference: **N264**

Specification description

Ø35mm ceramic sequential cartridge with base + collar.

Cartridge for wall-mounted basin mixers 2640, 2641.