4081N

**U-shaped toilet roll holder with spindle**

Reference: 4081N

Specification Description

U-shaped toilet roll holder with spindle in white, high strength polyamide (Nylon).

Ø 20mm tube.

Concealed fixings.

10-year warranty.