510580

**Wall-mounted liquid soap dispenser, 1 litre**

Reference: 510580

Specification Description

Wall-mounted liquid soap dispenser with soft-touch operation.

Vandal-resistant model with lock and standard DELABIE key.

One-piece hinged cover for easy maintenance and improved hygiene.

Push-button with soft-touch operation.

Anti-blocking: single dose per press, even if the button is pressed for prolonged periods.

Waste preventing, non-drip (waterproof) pump dispenser.

Tank with large opening: eases transfer of soap from large containers.

Tank prevents long-term stagnation of soap.

Window for monitoring soap level.

304 stainless steel, bright polished finish.

Stainless steel thickness: 1mm.

Capacity: 1 litre.

Dimensions: 90 x 105 x 252mm.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s.

Compatible with hydroalcoholic gel.

10-year warranty.